WEIGHT MASTER – SOLID SUPPORT IN TRANSPORT AND ON CONSTRUCTION SITES
The new version of the Wielton Weight Master construction tipper is part of the rear-tipping self-unloading semi-trailer range. Thanks to its aluminium body, its design is lightweight - starting from 4,560 kg - yet durable. It offers extended service life and a capacity ranging from 23 m3 to 64 m3. Designed for transporting bulk and agricultural materials, as well as asphalt, fuel, pallets and BIG BAG sacks, it is suitable for the construction, municipal and agricultural sectors.

The use of a straight frame made of S700MC steel, replacing the previous design tapered towards the front, has increased the vehicle’s strength. The new layout of the frame equipment components has been designed with greater ergonomics, easier operation and more efficient access to elements requiring inspection or technical servicing in mind. The fifth wheel plate and suspension components produced using hydroforming technology provide additional structural reinforcement, increasing chassis rigidity and thereby enhancing the stability and safety of the semi-trailer’s operation.

The rigidity of the load body is improved by new side wall profiles, which strengthen its structure 
and enhance the semi-trailer’s durability in everyday operation. By increasing the spacing of the main frame beams to 1,400 mm and the wheel track to 2,140 mm, as well as widening the spacing of the suspension air bags, the semi-trailer offers greater lateral stability. This solution is particularly important when raising the load body in difficult off-road conditions and when negotiating bends with a heavy load. During side-slope tests, the new version of the Weight Master semi-trailer achieved 
a result of 8°, qualifying it for Category A in accordance with IRTE guidelines.

The floor, made of highly durable aluminium alloy (ENDUR-AL. HB110), is designed to provide maximum resistance to abrasion. The use of a straight floor edge makes it possible to achieve an internal width suitable for transporting palletised loads. Depending on customer requirements, the semi-trailer can be equipped with a tailgate with or without a discharge hatch, a removable chute, or symmetrical barn doors with two discharge openings.

The proven solutions used in the Weight Master model - including the weight-optimised frame, new tarpaulin system, and stable, lightweight working platform in its new version, compliant with machinery standards - ensure safe transport and vehicle operation in all conditions. In addition, the tipper features a new bumper design folded using gas springs. Standard equipment includes, among others, an automatically lifted first axle and modern LED lighting. In addition to durability and functionality, the coating applied to the structure is also of key importance. Thanks to the use of a high-quality anti-corrosion coating, the manufacturer guarantees high corrosion resistance and an impeccable appearance throughout the entire operating life and in all conditions.

The applied solutions perform excellently in everyday use and meet the needs of even the most demanding users. Customers can choose the body capacity, floor length, type of closure and side wall profile thickness. The tipper produced by the Wieluń-based manufacturer can be configured in many ways, also thanks to a wide range of optional equipment, such as a third steering axle, sliding roof or metallic paint finish.
The new version of the Weight Master and other vehicles from the brands belonging to the Wielton Group can be viewed at the indoor stand E02 in Hall 27 and at the outdoor stands K41 and M67.
