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Domino Expands K300 High-Resolution Digital Inkjet Printing Solution with New High-Contrast White Ink
Direct-to-packaging coding solution supports high-quality, durable 2D code printing on a wide range of products and packaging materials.
Domino Printing Sciences (Domino) is pleased to announce the launch of a new high-contrast, high-performance white ink for its K300 digital inkjet printing solution. The new white capability provides greater flexibility in the application of high-quality variable data and 2D codes – including QR codes powered by GS1 – on a wide range of products and packaging materials, including multi-colored bottle caps and closures.
The K300 digital inkjet printing solution has been developed to support manufacturers with increasing 2D code requirements in complex production environments. The complete solution includes options for black, white, or dual black-and-white printing, integrated plasma pre-treatment, UV curing technology, and automated code verification, to deliver durable, high-contrast coding on a broad range of substrates.
“Manufacturing is becoming more complex across the board – changing consumer preferences are leading to an increase in product diversification, with many brands looking to manage multiple different products within existing manufacturing footprints,” says Toby Gugoașă-Hayhurst, Product Manager Digital Monochrome, Domino. “Our customers are also under pressure to print high-resolution variable data 2D codes for product traceability, regulatory compliance, and consumer engagement.”
“With the launch of our new white ink, manufacturers can manage complex, high-resolution coding requirements across a range of packaging types, shapes, and substrate colors within a single solution,” continues Gugoașă-Hayhurst.
The global shift to on-product 2D codes marks a major development in packaging identification that is driving the need for coding equipment that delivers high-contrast, high-resolution codes at high manufacturing speeds. At the same time, rising SKU counts are increasing production complexity. This is particularly relevant in sectors such as beverage, where manufacturers may need to manage multiple pack sizes and formats on a single line. Regulatory codes must meet strict industry grading requirements, deliver excellent contrast, and withstand supply chain pressures – including exposure to hot and cold environments. 

The K300 digital inkjet coding solution has been developed with these manufacturing challenges in mind, to deliver durable, high-resolution variable data 2D codes on a range of products and packaging types – including bottles, packages, labels, and flexible packaging. 
The K300 solution reliably prints variable data 2D codes at speeds of up to 250m per minute to meet the needs of high-speed production lines, including those in the beverage and FMCG sectors. The solution supports direct bottle cap printing through Domino’s Bottle Closure Printing Station, to support the move to labelless water bottles. Previously available with black ink, the addition of white ink enables high-contrast black-on-white coding on a wide range of colored caps and closures.
The complete K300 solution includes options for a single printhead or a dual solution, with the dual option capable of printing in both black and white ink, enabling manufacturers to manage a wide range of substrates and packaging types without requiring significant line changes. The solution can be integrated with plasma pre-treatment and UV LED curing solutions from Domino’s technology partners to help ensure durable codes that withstand the test of time. 
With a K300 digital inkjet printing solution, manufacturers have complete flexibility in managing 2D code requirements, with the option of printing direct-to-packaging, direct-to-product, or direct-to-label, with the possibility of integration into existing digital or flexographic printing solutions. Optional integration with Domino’s R-Series vision systems completes the solution by providing consistent code quality and scannability checks, helping reduce the risk of coding errors, recalls, and wasted stock.
“With the launch of our new white ink, we are pleased to offer one of the most comprehensive 2D code printing solutions available on the market, designed to enable manufacturers to embrace 2D coding across a broad range of packaging formats, colors, and substrates,” says Russell Wiseman, Global Beverage Sector Manager, Domino. “The complete K300 solution is the latest example of how Domino is committed to helping customers manage increasing variable data printing requirements and changing customer expectations while helping to maximise production efficiency.”
Discover how the K300 digital inkjet printing solution can help deliver high-quality variable data and 2D codes across a wider range of packaging formats and substrates.
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Information contained within this press release is considered to be true and correct at the date of publication by Domino, changes in circumstances after the time of publication may impact the accuracy of the information. All performance related figures and claims quoted in this document were obtained under specific conditions and may only be replicated under similar conditions. For specific product details, you should contact your Domino Sales Advisor. This document does not form part of any terms and conditions between you and Domino.

Notes to Editors:
About Domino
Since 1978, Domino Printing Sciences (Domino) has established a global reputation for the development and manufacture of coding, marking, and printing technologies, as well as its worldwide aftermarket products and customer services. Today, Domino offers one of the most 
comprehensive portfolios of complete end-to-end coding solutions designed to satisfy the compliance and productivity requirements of manufacturers across many sectors, including food, beverage, pharmaceutical, and industrial. The company’s core technologies include innovative inkjet, laser, print and apply, and thermal transfer overprinting systems designed for the application of variable data, barcodes, and unique traceability codes onto product and packaging. 
Domino employs over 3,000 people worldwide and sells to more than 120 countries through a global network of 29 subsidiary offices and more than 200 distributors. Domino’s manufacturing facilities are located in China, Germany, India, Sweden, Switzerland, UK, and the USA.
Domino became an autonomous division within Brother Industries Ltd. on June 11th, 2015. 
For further information on Domino please visit www.domino-printing.com 
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